**RISK ASSESSMENT INSPECTION REPORT**

Made on 16 March 2022 by Paul Elmhirst and Richard Daniel

Presented to Stillingfleet Parish Council on the 24 May 2022.

#### THE GREEN

|  |  |  |
| --- | --- | --- |
|  | **Problem** | **Recommended Action** |
| Trees | 1. SW corner – broken branch hanging down requires removal 2. Low branches on crack willow 3. Tree overhanging S Duggan’s garden | Branches Out to be reminded. Planning to remove has been granted  Letter sent to Selby in Nov or Dec – send reminder |
| Walls / fences / hedges | None |  |
| Manhole covers | Rusted manhole cover in NE sector of the Green | Write to possible residents responsible |
| Drain outlets | Undergrowth on banks of the beck make some outlets hard to locate | Make inspection after dredging has taken place |
| Effluent leaks | Possible leaks but Green is very wet at present – leaks will be easier to detect in dry conditions | Make summer inspection |
| Dog Poo | No immediate evidence but complaints are regular |  |
| Notices | Footpath sign on SW sector is broken | Already reported to NYCC |
| Other Stuff | Verge damage during development of Fearndale plot | Keep a close eye on road and verge damage by contractor |

#### THE PARISH FIELD

|  |  |  |
| --- | --- | --- |
|  | **Problem** | **Recommended Action** |
| Fences and gates | To be checked |  |

#### PERMANENT STRUCTURES

|  |  |  |
| --- | --- | --- |
|  | **Problem** | **Recommended Action** |
| Street lights | One still out outside Banbury House | Cllr Cook has this in hand |
| Bus shelters | None |  |
| Benches | None |  |
| Waste bins | None |  |
| Footbridges | Appears sound |  |
| Pavements | Reasonable but damage to verge of Green where construction is taking place | Contractor has agreed to rectify on completion of development. |
| Telephone kiosk | The telephone kiosk on York Road Stillingfleet is in a dilapidated state consistent with its age of some 85 or 90 years.  The door and its hinges seem sound.  On the right hand side (from the road) there are two small broken panes measuring 6”x2 1/2 “  On the left hand side there is one broken pane 6” x 2 1/2”.  At the front there is one missing pane 6” x 12”. The remaining panes are all plastic except for the top pane.  The kiosk has been leaning slightly to the left for at least 40 years without any sign of progressive movement. It is believed to be approximately 2” to 3” out of vertical and quite stable.  The paint work is peeling. | The Stiillingfleet Telephone Box Restoration Group is raising the funds to restore and refurbish the box |